Network Layers


Tatu Bogdan Gr. 3.1

1. 2 Extranet access users – EMAG







3. 5 Protocols




UDP: User Datagram Protocol




RTCP: Real-time Transport Control Protocol



MDNS: Multicast Domain Name System




ARP: Address Resolution Protocol




TCP: Transmission Control Protocol

4. Frame 720




Start acquisition time: 11.012321s from start

5. Frame 180



Frame size: 1392 bytes

6. Resolve MAC address setting



With:



Without:



Shows the manufacturer/vendor/host names based on the first 3 bytes of the MAC address